From f95d5d8da10151583dfc42e8d01e5286c88b4b61 Mon Sep 17 00:00:00 2001
From: Camil Staps
Date: Wed, 28 Sep 2016 22:51:12 +0200
Subject: Typesetting

---
 thesis/fix-storing-pc.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'thesis/fix-storing-pc.tex')

diff --git a/thesis/fix-storing-pc.tex b/thesis/fix-storing-pc.tex
index 4a203b3..fbc5853 100644
--- a/thesis/fix-storing-pc.tex
+++ b/thesis/fix-storing-pc.tex
@@ -61,7 +61,7 @@ This means that when the \ual{add} instruction above is at \ual{0x22},
 However, in this case \ual{bl} is located at \ual{0x2a}, and since this is a 32 bits instruction we point to the middle of that instruction.
 
 In hand-written code, we can solve this by adding labels for the addresses we want to store on the stack.
-In generated code, we need to keep track of the current alignment and add either \ual{9} or \ual{11} to the read program counter.
+In generated code, we need to keep track of the current alignment and add either 9 or 11 to the read program counter.
 
 \subsubsection{Other solutions}
 Another solution than the one we present here is the use of the link register.
-- 
cgit v1.2.3

