From e582e8e9d7e1b8e7025cfc4b58ba687491d3b3f2 Mon Sep 17 00:00:00 2001
From: Camil Staps
Date: Tue, 15 Nov 2016 23:45:33 +0100
Subject: Lot of formatting; rewriting storing-pc; references; natbib ->
 biblatex; autoref -> cref; minted; etc.

---
 thesis/two-bits.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'thesis/two-bits.tex')

diff --git a/thesis/two-bits.tex b/thesis/two-bits.tex
index 4b08d89..fcd4046 100644
--- a/thesis/two-bits.tex
+++ b/thesis/two-bits.tex
@@ -13,7 +13,7 @@ Instructions are halfword-aligned, so bit 1 is part of the address.
 Additionally, bit 0 is used to facilitate ARM and Thumb interworking.
 When the PC is written to with a value where the LSB is cleared,
 	the processor jumps and switches to ARM mode.
-When the LSB is set, it switches to Thumb mode~\citep[A2.3.2]{armv7ar}.
+When the LSB is set, it switches to Thumb mode~\parencite[A2.3.2]{armv7ar}.
 
 \subsection{Usage in Clean}
 \label{sec:two-bits:clean}
-- 
cgit v1.2.3

