\section{System setup}
\label{sec:system}

\begin{multicols}{2}

Tests were run on a Raspberry Pi 3, Model B with 1GB RAM.
Its processor is listed in \texttt{/proc/cpuinfo} as an `ARMv7 Processor rev 4 (v7l)',
	although the Hardware field is `BCM2709', which is an ARMv8 chip.

To build programs, we used the following suite:

\begin{itemize}[itemsep=0pt]
	\item gcc (Raspbian 4.9.2-10) 4.9.2
	\item GNU assembler (GNU Binutils for Raspbian) 2.25
	\item GNU ld (GNU Binutils for Raspbian) 2.25
	\item A Clean compiler built from intermediate ABC files retrieved on December 7, 2016 \parencite{cocl},
		built with the ARM code generator revision 295 \parencite{armcg}
		and the ARM RTS revision 387 \parencite{armrts}.
\end{itemize}

These programs are given \texttt{-march=armv7-a} when applicable to optimise for the ARMv7 architecture.
The Thumb backend proposed in this thesis uses features that are deprecated by ARMv8-A (see \cref{sec:intro:conditionals}).

\end{multicols}
